CAN Trace Analysis

This document outlines the process used to analyse CAN bus traces to investigate the feasibility of using dynamic CAN acceptance filtering.

Overview

The analysis consists of 4? Processes:

* Sequencing – The sequence order of valid ID’s in the CAN trace file is recorded.
* Timing – The time properties of each valid ID is calculated